Q1. Why can a frame loop endlessly in a switched environment with more than one way to a destination? (if spanning tree or a similar protocol is not enabled)

Q2. Are there any concerns with allowing auto-selection of the root bridge based on MAC addresses?

Q3. Please provide the shortest summary of PortFast you can.

Q4. Please provide the shortest summary of BPDU Guard you can.